DHCP-Dynamic host configuration protocol

In this exp I configured the router to dynamically allocate the address to the pc’s I connected in what range I want.