RIP stand for Routing Information Protocol. It is dynamic protocol.

RIP – Bellman Ford Algorithm

RIP – Max 16 Router

RIP – Send all Routing Table every 30 seconds

RIP – Administrative distance is 120

Metric – Hop count

Commands

#Router rip

#Version 2

#No auto-summary

#Network

#Network

I learnt how to configure RIP V2